2-2 Milestone One Submission

Joel Meza

Professor Ricky Sethi

January 11, 2022

CS 350 – Emerging Systems Architectures & Technologies

Southern New Hampshire University

**2-2 Milestone Submission: Q&A**

* **What does pwmled2 set the PWM period to?**
* The PWM (period) is to be set to three (3) milliseconds or three thousand (3,000) microseconds.
* **Which PWM\_xxx() function sets the PWM period?**
* The PWM\_(function) that sets the PWM period is called, “PWM\_Params\_init()”.
* **Which PWM\_xxx() function sets the PWM duty cycle?**
* PWM\_setDuty() is the function that is set to PWM duty cycle.
* **What is the purpose of the while(1) loop in pwmled2?**
* The purpose of the while(1) loop in pwmled2 is to load new edited and compiled code to iterate repeatedly until a manual response as (0) is known to stop the cycle.
* **What is the purpose of usleep() in the while(1) loop?**
* The purpose of the usleep(function) in the while(1) loop is to interrupt the execution in an interval time matter.